--- src/ntpd.8.orig	2017-09-07 19:12:02 UTC
+++ src/ntpd.8
@@ -56,7 +56,7 @@ Use
 .Ar file
 as the configuration file,
 instead of the default
-.Pa /etc/ntpd.conf .
+.Pa %%PREFIX%%/etc/ntpd.conf .
 .It Fl n
 Configtest mode.
 Only check the configuration file for validity.
@@ -99,18 +99,18 @@ will be logged.
 After the local clock is synchronized,
 .Nm
 adjusts the clock frequency using the
-.Xr adjfreq 2
+.Xr ntp_adjtime 2
 system call to compensate for systematic drift.
 .Pp
 .Nm
-is started at boot time by default via
-.Va ntpd_flags
+is usually started at boot time, and can be enabled by setting
+.Va openntpd_flags
 in
 .Pa /etc/rc.conf .
 See
 .Xr rc 8
 and
-.Xr rc.conf 8
+.Xr rc.conf 5
 for more information on the boot process
 and enabling daemons.
 .Pp
@@ -123,8 +123,8 @@ and its initial clock drift from
 .Pa /var/db/ntpd.drift .
 Clock drift is periodically written to the drift file thereafter.
 .Sh FILES
-.Bl -tag -width "/var/db/ntpd.driftXXX" -compact
-.It Pa /etc/ntpd.conf
+.Bl -tag -width "%%PREFIX%%/etc/ntpd.confXXX" -compact
+.It Pa %%PREFIX%%/etc/ntpd.conf
 Default configuration file.
 .It Pa /var/db/ntpd.drift
 Drift file.
@@ -134,12 +134,12 @@ Socket file for communication with
 .El
 .Sh SEE ALSO
 .Xr date 1 ,
-.Xr adjfreq 2 ,
 .Xr adjtime 2 ,
+.Xr ntp_adjtime 2 ,
 .Xr ntpd.conf 5 ,
+.Xr rc.conf 5 ,
 .Xr ntpctl 8 ,
 .Xr rc 8 ,
-.Xr rc.conf 8 ,
 .Xr rdate 8
 .Sh STANDARDS
 .Rs
