--- dox/netpipe.1.orig	2007-05-11 01:29:09.000000000 +0900
+++ dox/netpipe.1	2008-04-15 00:24:20.000000000 +0900
@@ -26,7 +26,7 @@
 .IB E valuator
 
 .SH SYNOPSIS
-.B NPtcp
+.B "NPtcp|NPtcp6"
 [\c
 .BI \-h \ receiver_hostname\fR\c
 ]
@@ -124,9 +124,9 @@
 
 
 
-.SH TESTING TCP
+.SH TESTING TCP/TCP6
 .PP
-NPtcp can now be launched in two ways, by manually starting NPtcp on
+NPtcp can now be launched in two ways, by manually starting NPtcp or NPtcp6 on
 both systems or by using a nplaunch script.  To manually start NPtcp,
 the NetPIPE receiver must be 
 started first on the remote system using the command:
@@ -147,7 +147,9 @@
 Any options used must be the same on both sides.  The \-P parameter
 can be used to override the default port number.  This is helpful when
 running several streams through a router to a single endpoint.
-
+.PP
+The NPtcp6 program is launched in a similar manner.
+.PP
 The nplaunch script uses ssh to launch the remote receiver
 before starting the local transmitter.  To use rsh, simply change
 the nplaunch script.
@@ -376,6 +378,11 @@
 .ne 3
 
 .TP
+.BI \-P \ \fIport\fR
+Set the port number used by the TCP and TCP6 tests to \fIport\fR.
+.ne 3
+
+.TP
 .B \-r
 This option resets the TCP sockets after every test (TCP module only).
 It is necessary for some streaming tests to get good measurements
